=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-MAR-94 :
data up to 1992 revised, March 1994
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 18-Sep-2008 :
RLR calculated for this station 17.9.08
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Sep-2011 :
Primary benchmark remains 79L003 21.571m above TGZ
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2014 :
The tide gauge at Port Alfred is currently not operational. We have been informed that there are no plans at this time to have it back on the network.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Jul-2015 :
This year, rather than just sending the latest year of data the complete dataset has been supplied. This has highlighted some differences in the data. From communications in the correspondence file for 2002 it appears that the Oceans and Fisheries meant to supply revised data for the stations supplied. This did not happen. The complete dataset includes these data revisions. Therefore, the whole dataset has now been re-entered.
The tide gauge at Port Alfred has now been removed.

