=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-MAY-96 :
Revised data up to 1985 supplied by the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Aug-2010 :
Supplying authority have confirmed the measurement datum is LAT, and the primary tide gauge bench mark HR1 is 3.887 m above LAT from 1987 onward. RLR (2009) has been defined as 10.2 m below HR1

