=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Oct17 :
The gauge is an Aanderaa WLR7 tide recorder.
The gauge is installed along the wharf of
Port-aux-France.  This bottom pressure sensor
is at the base of a stilling well which is
used to filter waves.  The recorder is
triggered by a central unit where the barometric
pressure is measured at the same time.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Nov05 :
Monthly means fully corrected for air pressure drift effects have been
used from the French operators.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 22-Sep-2010 :
Kerguelen is part of the French Rosame network. Data for April 1993-May 2010
was downloaded from ftp://ftp.legos.obs-mip.fr/pub/soa/niveau_mer/rosame/.
Data for May 1993- Dec 2000 was already in the database the new data appears to
be a month out of phase with the old but agrees with the Hawaii data. Previous
data has been stored.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Feb-2014 :
Laurent Testut for LEGOS the authority responsible for Kerguelen suspects that the data displayed on the SONEL website is infact the unreferenced data. He is going to investigate the situation and confirm.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2014 :   
Using values from the SONEL website the latitude and longitude for Kerguelen has been revised.

