=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Kapingamarangi      710/026 RLR(1984) is 8.6m below BM#1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-OCT-91 :
Daily and hourly residuals show significant fluctuations with duration of around a day associated with Westerley winds. Silting around the stilling well caused fluctuations in 1987-1989.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 13-MAY-94 :
Silting around the stilling well caused questionable fluctuations 1987-90
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-OCT-96 :
Gauge type: Leupold and Stevens Analog-to-Digital Recorder (ADR);(Jul 1985-present) Handar Encoder (ENC)
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 1998Dec31 :
Data for 1996 revised in December 1998
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-Nov-2010 :
The complete dataset 1978-2008 has been supplied by UHSLC. After checking with existing data values these were loaded onto the database. Values for Nov 2000 onwards are 3-4mm lower than previous values. Previous data were flagged Jan 1987-Dec 1989 see above. The flags have been replaced with a station flag. RLR remains 6.037m.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Oct-2015 :
Using the latest JASL data the complete dataset has been reloaded. Referring to the UH levelling information it is clear that the RLR diagram was prepared using the 1978 levelling value of 2.563m for benchmark UH-1.This remained stable within +2mm before being destroyed. The remaining stable benchmark in the 1996 and 2000 levelling is BM @ which relates to the tide staff. This has been added to the RLR diagram.

