=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Oct17 :
Tide gauge is an Aanderaa WLR7 tide recorder.
The gauge is installed in the crater of a
partially submerged volcano, communicating
with the open ocean through a narrow (100m)
and shallow (2m at low tide) pass.  This bottom
pressure sensor is at the base of a stilling well
which is used to filter waves.  The recorder is
triggered by a central unit where the barometric
pressure is measured at the same time.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Oct17 :
All monthly means for Saint Paul have been taken from the University of
Hawaii Sea Level Center to which data are directly relayed by the
French operators.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 22-Sep-2010 :   
Saint Paul is part of the French Rosame network. Data for Oct 1994- Dec2006
were downloade from ftp://ftp.legos.obs-mip.fr/pub/soa/niveau_mer/rosame/.
Previously held data Nov 1994- May 2000 looks almost the same and has been
stored.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-Oct-2014 :   
Using data from SONEL the latitude and longitude for Saint Paul has been updated.

