=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2000May10 :
Float type gauge , installed 1999.  Digitised record.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Jun04 :
Skopelos            290/037 RLR(2000) is 8.760m below R69(YY)
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Aug-2013 :   
Benchmark R 69 YY no longer exists. Benchmark now R 20 0.48m above zero level
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-Aug-2016 :   
The supplying authority the Hellenic Navy Hydrographic Service has recently confirmed that the tide gauge at Skopelos is currently out of order due to gauge malfunction.

