=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 17-MAY-96 :
Data up to 1960 supplied by Queensland D.O.T. Revised data for 1960-1979 received from the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010 :
Data supplier the NationalTidal Centre has confirmed that tide gauge zero from 1960 is LAT. Benchmark PSM 10043 is 9.916 m above LAT. RLR (2009) is defined as 13.9 m below PSM 10043

