=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-APR-96 :
Revised data for March/April 1996 received from the National Tidal Centre, Bureau of Meteorolgy, South Australia.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 15-JAN-98 :
Revised data for 1994-1995 received from the National Tidal Centre, Bureau of Meteorology, South Australia.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-JAN-98 :
Gauge type=Druck (pressure) and Aquatrak (acoustic) transducers both pressure transducers are installed at Garden Cove

