=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Daeheug San Do      620/028 RLR(1979) is 10.6m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-FEB-93 :
gauge resited 1979
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Daeheug San Do      620/028 RLR(1979) is 10.6m below TBM No2
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-DEC-97 :
Type of tide gauge: OTT float
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012 :
At the request of the data suppliers, KHOA the station name has been corrected
to Daeheuksando. The lat. and long. have also been revised.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Aug-2012 :
From historic documentation on the old RLR diagram when preparing the revised
diagram for the website the RLR factor was changed from 5.131m to 5.132m.

