=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
Data for 1961-1962 was supplied by Australian Ocean Data Centre N.S.W.These data are based on High and Low water readings.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 13-NOV-91 :
Data for 1969 was supplied by the National Tidal Centre, Bureau of Meteorology, South Australia based on hourly values
========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-MAR-96 :
Revised data for 1985-1990 was supplied by the National Tidal Centre, Bureau of Meteorology, South Australia. SEAFRAME station installed 04/09/92. Cocos (Keeling) Is. is a cooperative station between NTF and NOAA/NOS
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-JAN-98 :
1985-1992: gauge type=Float/well system Stevens analog-to-digital recorder
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-JAN-98 :
1961-65: float/stilling well gauge located on original jetty West Is. 1968-71 float/stilling well gauge located near jetty, West Is.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2000Apr10 :
This is a "baseline station" of the Australian National Tidal Facility.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2000Apr10 :
Cocos Is.(Home Is.) 680/521 RLR(1996) is 8.604 below PSM101
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 27-Oct-2011 :
Using metadata from the National Tidal Centre, Australia the RLR diagram has been revised. Primary benchmark is SEAFRAME sensor benchmark 3.554m above Tide Gauge Zero (TGZ). RLR factor is 6.20m.

