=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-MAY-96 :
Revised data 1982-1986 recived from the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 23-Aug-2010 :
Supplying authority have confirmed that for data after 9/10/1982, vertical datum is Chart Datum. Primary benchmark A 958 is 7.477 m above Chart Datum. RLR (2008) defined as 11.6 m below
A 958
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-Mar-2013 :
The reference datum for King Bay changed from Chart Datum to Lowest Astronomical Tide (LAT) on 01/01/2009. The differece between the two is 0.12m the RLR factor has changed.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 19-Aug-2013 :
Following a recent download of data for King Bay from the NTC website it was noticed that the data for 2008 had been revised. This data has now been re-loaded onto the database.

