=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010 :
Data supplier confirmed tide gauge benchmark PSM 8295 is 5.103 m above tide gauge zero (LAT). RLR (2009) has been defined as 10.2 m above PSM 8295

