=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 13-JAN-98 :
National Tidal Facility SEAFRAME station
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 25-Aug-2010 :
Supplying authority have confirmed tide gauge benchmark KIR 1 is 3.5334 m above tide gauge zero.RLR (2009) is defined as 8.8 m below KIR 1

