=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-JAN-98 :
Lombrum is an NTF SEAFRAME station
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 21-JAN-98 :
1995 (April-Dec): gauge was decommissioned while the jetty was repaired
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 25-Aug-2010 :
Supplying authority has confirmed that benchmark PNG 1 is 2.2988 m above tide gauge zero.RLR (2008) is defined as as 8.5 m below benchmark PNG 1

