=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Zlarin              280/017 RLR(1985) is 9.3m below BM
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Zlarin              280/017 RLR(1985) is 9.3m below BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-JAN-96 :
gauge discontinued 2 June 1988

