=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2002Sep24 :
A description of the sea level network in Finland can be found
in 'Operational Oceanography: Implementation at the European
and Regional scales.  2002 (pp.129-137)'.
PRIOR TO 1971 FCODE=06
PRIOR TO 1983 GAUGE AT 61 08 N, 21 27 E
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Rauma/Raumo         060/121 RLR(1964) is 7.7m below BMP3
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Rauma/Raumo         060/121 RLR(1964) is 7.7m below BMP3
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 09-Jan-2012 :   
The tide gauge at Rauma was moved during 1983. Levelling information recently
supplied by the Finnish Meterological Institute confirms that benchmark P3 no
longer exists. Primary benchmark is now 92403 4.089m above the gauge datum.

