=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Dubrovnik           280/081 RLR(1964) is 11.3m below BM
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 04-MAR-92 :
Prior to 1990 data from Hidrografski Institut, Split
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-JAN-96 :
Tide gauge of the State Hydrographic Institute at Split
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-JAN-96 :
Gauge=A. Ott, Kempten
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Jan-2011 :
The tide gauge at Dubrovnik has been operational since 1956.Following receipt of a station information sheet: Primary benchmark is R1 5.333. above TGZ. Secondary benchmark is A 496 4.789 above TGZ. RLR factor is 5.967m.

