=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2002Jan09 :
For an analysis of sea level changes in Hong Kong, see
"Sea level changes in Hong Kong from tide gauge measurements"
by X.Ding et al., Journal of Geodesy, 74, 683-689, 2001 and
"Long-term sea-level changes in Hong Kong from tide-gauge
records" by X.Ding et al., Journal of Coastal Research,
17, 749-754, 2001.
BEFORE 1986 DATA SUPPLIED BY AUTHORITY NO. 40
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Chi Ma Wan          611/008 RLR(1963) is 27.5m below BM at 4A
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Chi Ma Wan          611/008 RLR(1963) is 27.5m below BM at 4A
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 09-Oct-2012 :   
This is now an historic station.Last data 1997.

