=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Port Irene          660/003 RLR(1992) is 10.6m below BM 1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 1999Mar30 :
gauge type = Ott
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-Oct-2009 :   
2006 is the last data received from Port Irene as the
tide gauge has been removed due to development of the pier.
A replacement gauge has been established at San Vicente.

