NOTICEABLE METEOROLOGICAL INFLUENCES
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Mar del Plata(Club) 860/101 RLR(1977) is 11.8m below Repere No 11
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Mar del Plata(Club) 860/101 RLR(1977) is 11.8m below Repere No 11
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 1999Aug20 :
station is equipped with both float gauge and NGWLMS system
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Mar21 :
Acoustic gauge installed 1992, alongside existing float gauge.
Mid 1998 - tide gauge found to be left dry after dredging works.
May 1999 gauge relocated 5km south, within Naval Base.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2002Jan09 :
Mar del Plata (Club) gauge (38 03 S, 57 33W) moved to
Mar del Plata (Naval Base) (38 02'S, 57 31'W) December
1998 because of beach works.  New site levelled into
old benchmark (Repere No.11) and data treated as continuous.

