=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-MAY-96 :
Revised data for 1985-1986 received from the National Tidal Centre, Bureau of Meteorology, South Australia
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Aug-2010 :
Data supplier have confirmed tide gauge zero of datum is Chart Datum, and benchmark DOT 001 is 3.499 m above Chart Datum. RLR (2008) has been defined as 8.8 m below DOT 001

