=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Rodbyhavn           130/011 RLR(1964) is 7.8m below original BMK-31-9011
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-APR-92 :
New installation January 1991
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 07-JUL-92 :
Prior to 1991 fcode=24
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Feb-2008 :
Previously held data for 2000-2002 revised using values supplied by DMI. Data for 2003-2006 also supplied.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Oct-2012 :
Information from DMI confirms Primary benchmark now G.I. 1610 0.780m above TGZ.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 12-Sep-2013 :
The PSMSL has received Thechnical Report 13-15 'Sea level data 1889-2012 from 14 stations in Denmark Mean, maximum and minimum values calculated on monthly and yearly basis including plots of mean values' from the DMI. As a result of the exercise data values for Rodbyhavn 1980-2012 have been revised. These revised data values have been entered onto the database.

