=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Ulneung Do          620/059 RLR(1982) is 10.0m below TBM No3
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Ulneung Do          620/059 RLR(1982) is 10.0m below TBM No3
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 08-DEC-97 :
Type of tide gauge: OTT float
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-Jul-2012 :
At the request of the data suppliers, KHOA the name for this station has been
changed to ULLEUNG. The values of the lat. and long. have also been revised.

