=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 1999Sep03 :
Acoustic gauge (Aquatrak 4100 series sensor) installed in April 1999
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2000Jun05 :
New analogue chart, float gauges were installed in 1985 in 4 Turkish
stations: Antalya II, Bodrum II, Metes/Izmir and Erdek. All were
replaced by new acoustic systems in 1998-99.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2000Jun05 :
Mentes              310/042 RLR(1995) is 8.794m below BM MAR 1
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-Jun-2010 :   
Mentes is on the Aegean Sea. This station forms part  of the Turkish Sea Level
Monitoring Network. The total dataset has been revised by the authority.
Therefore a new RLR diagram was created. RLR (2006) is 8.000m below TGBM
MNTS-1. RLR factor is 5.244m.

