Data from 2 sites prior to 1959 MSL values based on readings of high and low waters.Data prior to 1962 referred to BM which has proved unstable irregularities in records for 1940 & 1941. 1940-41. Data therefore ommitted gauge at new site in September 1965.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Lagos               210/031 RLR(1974) is 10.0m below BMOP
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-AUG-92 :
The 1941 irreularities may be connected with the 1941 earthquake - See Bottari et al. , tecttonophysics 202, 269-275, 1992 and Yamguti, R.Soc.New Zealand bulletin , 9, 127-128, 1971.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 14-JAN-97 :
Data for 1985-88 revised, January 1997
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Mar28 :
Data for 1986-87,90-92,95,99 updated March 2001 Lagos is an historic station last data 1999
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 22-Jan-2016 :
A value of MTL-MSL=7 mm has been applied to the RLR data for the period 1908-1958.  This value was derived by Philip Woodworth in preparation of his MTL/MSL manuscript.  In this case the values were derived using from the GESLA2 (high-frequency tide gauge) dataset using harmonic constituents.

