=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Oct17 :
The gauge type is a MORS (bottom-mounted pressure gauge).
The tide gauge is installed in the Baie du Navire,
Possession Island, in the Crozet archipielago,
nearby the Alfred Faure french scientific base.
The gauge is a MORS automatic tide gauge station
and consists of a ventilated ParoScientific
pressure sensor at the base of a stilling well
which is used to filter waves.  The ventilation
of the sensor results in a measurement of the
total pressure (atmosphere + ocean) minus the
atmosphere; hence, a direct measure of sea level,
assuming water density is properly estimated.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2001Oct17 :
All monthly means for Crozet have been taken from the University of
Hawaii Sea Level Center to which data are directly relayed by the
French operators.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 26-Feb-2014 :
Following information received from LEGOS the authority responsible for the Crozet tide gauge. They have confirmed that the gauge is not yet levelled into any benchmark.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Sep-2014 :   
Using values from the SONEL website the latitude and longitude values for Crozet have been revised.

