=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Aarhus              130/081 RLR(1964) is 11.0m below BMGM898
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Feb-2008 :
Previously held data for 2000-2002 revised using values supplied by DMI. Data for 2003-2006 also supplied.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Oct-2012 :
Information from DMI confirms Primary benchmark remains G.M.898 3.988m above TGZ.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Sep-2013 :
The PSMSL has received a copy of Technical Report 13-15 'Sea level data 1889-2012 from 14 stations in Denmark Mean, maximum and minimum values calculated on monthly and yearly basis including plots of mean values' from the DMI. As a result of the exercise data values for Aarhus 1970-2012 have been revised. The revised data values have been loaded onto the database.

