=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 02-MAY-95 :
Station density along some sections of the Australian coast has meant that station codes 601 onwards have been re-ordered compared to those in earlier versions of the PSMSL data set.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 28-MAR-96 :
Revised data received from the National Tidal Centre, Bureau of Meteorology, South Australia. SEAFRAME station installed 13/03/1992
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2000Apr10 :
This is a "baseline station" of the Australian National Tidal Facility.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 2000Apr10 :
Esperance           680/446 RLR(1996) is 11.043m below ZI/73
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 24-Oct-2011 :
Benchmark Z1/73 is 4.743m above TGZ. Benchmark TIDE ESPERANCE is 4.782m above TGZ. The national datum reference AHD is 0.707m above TGZ. The RLR factor is 6.3m.

