=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Andenes             040/041 RLR(1955) is 7.3m below FM AndenesI
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Andenes             040/041 RLR(1955) is 7.3m below FM AndenesI
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-OCT-93 :
DATA UP TO 1986 FROM AUTHORITY CODE 03
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-MAR-95 :
tide gauge network modernised, new equipment installed in 1991
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 06-Apr-2009 :   
2007/8 mean sea level values entered as METRIC only
awaiting confirmation of a datum query.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 19-Jul-2010 :   
The Norwegian Mapping Authority has revised all its datasets. The Primary bench
mark for Andenes from 1991 onwards is L7 N42which is 5.245m above TGZ (See copy
of the page for
Andenes from the Norwegian website with the RLR diagram). RLR has been
re-calculated using 2008 as the RLR year. Revised RLR factor is now 5.055m from
1991 data onwards. RLR (2008) is 10.3m below TGBM L7 N42.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 05-Sep-2012 :   
For information on sea level change along the Norwegian coast see paper
"Contributions to sea level variability along the Norwegian coast for 1960-2010"
by K.Richter, J.E.O. Nilsen and H. Drange.

