=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Esbjerg             130/121 RLR(1964) is 22.0m below BMGM879
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-APR-92 :
New installation February 1991
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 29-JUL-93 :
Anomalously low value February 1947 - correct as received from authority.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Feb-2008 :
Previously held data for 2000-2002 revised using values supplied by DMI. Data for 2003-2006 also supplied.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 20-May-2010 :
Data values for 1991 were replaced by revised data values supplied by DMI.Previous values printed off and held in file.See letter of 16th March 2010.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 03-Oct-2012 :
Information from DMI confirms Primary benchmark remains G.M. 879 15.088m above TGZ.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-Sep-2013 :
The PSMSL has received a copy of Technical Report 13-15 'Sea Level data 1889-2012 from 14 stations in Denmark Mean, maximum and minimum values calculated on monthly and yearly basis including plots of mean values' from DMI. As a result of the exercise the full dataset for Esbjerg has been revised. The revised data values have been loaded onto the database.

