=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUN-91 :
Trondheim           040/141 RLR(1964) is 10.4m below BM"Sodemannsgt"
=========================== BENCHMARK INFORMATION UPDATE ADDED  12-JUL-93 :
Trondheim           040/141 RLR(1964) is 10.4m below BM"Sodemannsgt"
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 11-JUL-94 :
Anomalously low values July-September 1971 correct as received
from authority.
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 10-OCT-94 :
new gauge established in December 1989 but treated as separate
station (040/142) as no connection between old and new bench marks
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-MAR-95 :
prior to 1978 fcode=hl
=========================== FOLLOWING PSMSL DOCUMENTATION ADDED 30-MAR-95 :
tide gauge network modernised, new equipment installed in 1989
Trondheim is an historic station last data 1989

