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1.1 Noise & vibration
Please describe in the box below all measures that will be implemented to minimise the potential impact of noise & vibration on wildlife. Table 1 gives examples of measures which may be appropriate.
	


. 
1.2 Dust
Please describe in the box below all measures that will be implemented to minimise the potential impact of dust or other particulates on nearby sensitive sites, particularly watercourses and woodland. Such measures could include water spraying, enclosures or screening.
	



1.3 Pollution of watercourse
Please describe in the box below all measures that will prevent contamination of nearby watercourses from your operations. Such measures must include: 
· storage arrangements for chemicals
· your emergency procedure in the event of contamination, and 
· your incident reporting procedure. 
Table 2 gives examples of other measures which may be appropriate.
	



2. Use of plastics
If you are installing plastic piling or other plastic structures alongside a watercourse or near a sensitive site, please describe in the box below all measures that will prevent contamination of these features from micro-plastics. 
Table 3 gives examples of measures which may be appropriate. 
	



3. Waste management
Please describe in the box below how all waste, including foul water, will be managed or disposed of during the construction and operational phase of the development to minimise impact on the local environment. 
	



4. Lighting
Please describe in the box below any lighting measures, including security lighting, that will be implemented to minimise impact on sensitive nocturnal species, particularly bats, during construction works. 
Table 4 gives examples of measures which may be appropriate.
	



Tables
Table 1
Examples of mitigation measures to protect habitats and species from the impacts of noise and vibration: 
	Maintaining all vehicles and plant in good and efficient working order, and in accordance with manufacturer’s specification.

	Fitting all vehicles, mechanical plant, and machinery used with proper and effective silencers where available.

	Shutting down all plant and machinery in the intervening periods between works.

	Restricting duration of use of plant and machinery capable of generating significant noise and vibration levels.

	Siting static plant and machinery as far away as possible from noise sensitive locations such as nature reserves or SSSIs.

	Using mains electricity or battery powered equipment instead of diesel- or petrol-powered generators.

	Handling of materials in such a manner that minimises noise, including minimising drop heights into hoppers and lorries.

	Installing screening to reduce noise disturbance beyond the development site boundary.

	Timing of works to avoid most sensitive breeding, spawning or hibernating periods.



Table 2
Examples of mitigation measures to protect watercourses from chemical and particulate pollution (excluding micro-plastics – see Table 3):
	Limiting topsoil removal as required and covering topsoil whilst stockpiled.

	Cleaning machinery in designated areas with a sump and re-using wastewater where possible or discharging via a sewer or tanker only.

	Storing chemical and fuels securely within double-bunded bowsers or chemical stores (with a 110% capacity to contain any spillage.)

	Using a coffer dam to allow the controlled pouring of concrete or use of a preformed concrete section should the slipway extend into the river channel beyond the existing wall line.

	Using water based, non-toxic and biodegradable chemicals and fuels where possible.

	Mixing and washing chemicals and associated equipment in designated areas with wastewater safely disposed of via mains sewerage or tanker as appropriate.

	Regularly checking equipment (e.g. hydraulic pipes) for failures and/or leaks.

	Spill kits and booms present on the site and staff are trained in their use.

	Installing silt curtains to prevent sediment from dredging operations affecting sensitive habitats.



Table 3
Examples of mitigation measures to protect watercourses from plastic pollution:
	Only installing sheet piling that is intact and fit-for-purpose alongside a watercourse.  

	Ensuring physical integrity of the sheet piling is maintained through careful installation methods.  

	Cutting plastic sheet piling offsite or at a suitable distance from the water’s edge to ensure plastic residue is not blown or washed into the watercourse.  

	Preventing plastic waste entering the water through suitable containment measures and removing waste from site as soon as practical.  

	Installing a suitable depth of waling (or other buffering measure) and width of capping to prevent damage to the plastic piling. 

	Reinforcing plastic sheeting with timber or steel piles to maximise strength and longevity.

	Backfilling sheet piling to provide maximum strength.



Table 4
Examples of mitigation measures to protect nocturnal species from light pollution during construction works:
	Avoiding the use of artificial lighting between dusk and dawn. 

	Keeping lighting to the minimum level required for safety or security purposes to ensure the retention of a dark corridor.

	Screening of security lighting if night-time work required.
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